ABSTRACT

Implement Computed Tomografi ( CT ) Scan is an diagnostic supporter radiology appliance using X-Ray of through modern technique Tomografi computerization and representing health appliance which can be used to analyse all body organ in more accurate because in pelaksanaanya Save sinar-x from this implement make a move to turn around at perpendicular plane at body pasien.Irisan axis can be made depend on thick bind [released] ray, also apart between slice can be adapted for a checked body anatomy circumstance.
What implement Can CT-SCAN of simulation by using Mikrokontroller which can menyinpan and take data such as those which there is Implement of CT-SCAN in determining process work Gantry and Desk of patient without using Computer but using Network mikrokontroller .
Therefore the module which we make simulation of implement of CT-SCAN base on Mikrokontroller which used as a process work implement of CT-SCAN provided with setting of Position early, Amount Slice, Thick of Slice presented at LCD where in simulation work Gantry use censor of saklar of glass used to detect each;every rotation of gantry showing existence sum up slice joined with appearance LCD .
Pursuant to result of tally of slice at every settingan with mistake factor ( error) 0% because appearance at LCD show same number. While result of measurement of speed of gantry from result of mean of entirety of settingan [is] by mistake factor(error) 382% and result of uncertainty is 0,025 this because of in usage of motor of gantry use Motor of Gearbox having compared to slower speed motor of ordinary AC.
Simulation of Gantry and Desk of Patient at Implement of CT-SCAN can facilitate operator in execution and exploiting use Implement CT-SCAN